{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":1,"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":9,"rows_kept":5,"merged":[[0,0,0,8],[1,0,1,8],[4,2,4,6]],"flags":["formulas_cached_only"]}
["密集架"]
[]
["序号","图片","产品名称","规格","单位","数量","单价（元）","金额","商务要求及参数"]
[1,null,"密集架                   ","2400*900*560","仓",40,1740,69600,"*材质：优质一级冷轧钢板，材料、工艺符合国家标准。                                                                                                                                                           *地轨采用3.0mm厚U型钢，轨道采用20×20实心方钢，底梁、轴承档、夹紧块采用3.0mm热轧钢板，立柱采用1.8mm冷轧钢板，层板采用1.2mm冷轧钢板，挂板采用1.2mm冷轧钢板，防尘板采用1.2mm冷轧钢板，门框采用1.2mm冷轧钢板，门板采用1.2mm冷轧钢板，挡书条1.2mm冷轧钢板，轨道斜坡1.5mm厚冷轧钢板，柜门设加强筋，定位模块采用ABS，侧面板钢制侧护板采用1.2mm冷轧钢板，每组分12层板,每层两面均可以放档案。每块层板配加强筋，可上下自由移动，稳固性强。                                                                                            各部位的安装牢固、可靠、无松动现象。层板载荷能力≥150kg。符合 GB/T3325-2008、GB5296.2004 国家标准，在全负载的情况下，承受X、Y 轴向的水平拉力，拉力≥120 牛。\n传动机构：轴承采用P204E级，传动轴采用Ø2045#圆钢，连接钢管采用25×2.5无缝钢管，滚轮采用HT20-40铸铁，链轮采用ZG45精致齿轮，链条采用节距12.7滚珠链条，摇手体总成由ZG45摇手体和滚珠轴承组成。\n标示装置：指示清晰，可详细列明储存内容、方便文件分类及查寻。\n中央制锁装置：制动装置由808锁边列锁定装置和中间列制动装置组成。\n防护装置：防震、防尘装置采用20mm磁性吸条，防尘板、顶板采用1.2mm冷轧钢板，防鼠板采用1.2mm冷轧钢板。\n*防倾倒装置：采用4.0mm热轧钢板，将轴承装置在尾仓底，安装在路轨上，防止密集架侧倒伤人。\n底盘：采用高强度桥梁插接组合结构，立式调心轴承、双驱动双向传动、结构紧凑。                                                                                                                                               *房间地面要求：为增加房间承载力，房间地面均整体铺设12mm厚实芯钢板，钢板下面四周焊接实厚0.5mm厚10cm*5cm方钢，方钢四面插入墙体5公分深，满焊焊接，不划手，焊接点打磨平整。钢板表面铺原木色木地板，房间面积为35平米。\n地轨装防撞斜坡，铺设于地轨两侧，防止人.车过往不便。\n方钢地轨：采用壁厚3.0mm钢板"]
[2,null,"合计",{"$nulls":4},69600]